# Waveform formats
*.vcd
*.vpd
*.evcd
*.fsdb

# Default name of the simulation executable.  A different name can be 
# specified with this switch (the associated daidir database name is 
# also taken from here):  -o <path>/<filename>
simv

# Generated for Verilog and VHDL top configs
simv.daidir/
simv.db.dir/

# Infrastructure necessary to co-simulate SystemC models with 
# Verilog/VHDL models.  An alternate directory may be specified with this
# switch:  -Mdir=<directory_path>
csrc/

# Log file - the following switch allows to specify the file that will be
# used to write all messages from simulation:  -l <filename>
*.log

# Coverage results (generated with urg) and database location.  The 
# following switch can also be used:  urg -dir <coverage_directory>.vdb
simv.vdb/
urgReport/

# DVE and UCLI related files.
DVEfiles/
ucli.key

# When the design is elaborated for DirectC, the following file is created
# with declarations for C/C++ functions.
vc_hdrs.h
